    PAD Specification File
    ***************************

    PART TYPE:        LAV-AT-X70
    Performance Grade:      3
    PACKAGE:          LFG1156
    Package Status:                     Advanced       Version 28

    Thu Mar 14 15:43:21 2024

    Pinout by Port Name:
    +-----------+----------+--------------+-----------+---------------------------------------------------------------------------------------------------------------------------------------------------------------+
    | Port Name | Pin/Bank | Buffer Type  | Site      | Properties                                                                                                                                                    |
    +-----------+----------+--------------+-----------+---------------------------------------------------------------------------------------------------------------------------------------------------------------+
    | clk_in    | T7/0     | LVCMOS33_IN  | WRIO0_3B  | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN VREF:OFF        |
    | seg1      | R19/13   | LVCMOS33_OUT | WRIO13_0A | DRIVE:50RSmA SLEWRATE:SLOW GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE VREF:OFF |
    | seg2      | R18/13   | LVCMOS33_OUT | WRIO13_0B | DRIVE:50RSmA SLEWRATE:SLOW GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE VREF:OFF |
    | seg3      | R14/13   | LVCMOS33_OUT | WRIO13_1A | DRIVE:50RSmA SLEWRATE:SLOW GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE VREF:OFF |
    | seg_a     | T18/13   | LVCMOS33_OUT | WRIO13_2A | DRIVE:50RSmA SLEWRATE:SLOW GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE VREF:OFF |
    | seg_b     | T19/13   | LVCMOS33_OUT | WRIO13_2B | DRIVE:50RSmA SLEWRATE:SLOW GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE VREF:OFF |
    | seg_c     | T15/13   | LVCMOS33_OUT | WRIO13_3A | DRIVE:50RSmA SLEWRATE:SLOW GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE VREF:OFF |
    | seg_d     | U16/13   | LVCMOS33_OUT | WRIO13_4A | DRIVE:50RSmA SLEWRATE:SLOW GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE VREF:OFF |
    | seg_dp    | R15/13   | LVCMOS33_OUT | WRIO13_1B | DRIVE:50RSmA SLEWRATE:SLOW GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE VREF:OFF |
    | seg_e     | U17/13   | LVCMOS33_OUT | WRIO13_4B | DRIVE:50RSmA SLEWRATE:SLOW GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE VREF:OFF |
    | seg_f     | W14/13   | LVCMOS33_OUT | WRIO13_5A | DRIVE:50RSmA SLEWRATE:SLOW GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE VREF:OFF |
    | seg_g     | V14/13   | LVCMOS33_OUT | WRIO13_5B | DRIVE:50RSmA SLEWRATE:SLOW GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE VREF:OFF |
    | sw12      | V16/13   | LVCMOS33_IN  | WRIO13_6A | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN VREF:OFF        |
    | sw13      | V15/13   | LVCMOS33_IN  | WRIO13_6B | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN VREF:OFF        |
    | sw14      | T13/13   | LVCMOS33_IN  | WRIO13_7A | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN VREF:OFF        |
    | sw15      | R13/13   | LVCMOS33_IN  | WRIO13_7B | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN VREF:OFF        |
    +-----------+----------+--------------+-----------+---------------------------------------------------------------------------------------------------------------------------------------------------------------+

    Vccio by Bank:
    +------+-------+
    | Bank | Vccio |
    +------+-------+
    | 0    | 3.3V  |
    | 13   | 3.3V  |
    +------+-------+

    Vref by Bank:
    +------+-----+-----------------+---------+
    | Vref | Pin | Bank # / Vref # | Load(s) |
    +------+-----+-----------------+---------+
    +------+-----+-----------------+---------+

    Pinout by Pin Number:
    +----------------------------------+-----------------------+------------+--------------+--------------------------------+----------------------------------------+
    | Pin/Bank                         | Pin Info              | Preference | Buffer Type  | Site                           | Dual Function                          |
    +----------------------------------+-----------------------+------------+--------------+--------------------------------+----------------------------------------+
    | A5/55                            |                       |            |              | MPQ5_RX2P                      |                                        |
    | A6/55                            |                       |            |              | MPQ5_RX2N                      |                                        |
    | A8/55                            |                       |            |              | MPQ5_RX0P                      |                                        |
    | A9/55                            |                       |            |              | MPQ5_RX0N                      |                                        |
    | A11/54                           |                       |            |              | MPQ4_RX2P                      |                                        |
    | A12/54                           |                       |            |              | MPQ4_RX2N                      |                                        |
    | A14/54                           |                       |            |              | MPQ4_RX0P                      |                                        |
    | A15/54                           |                       |            |              | MPQ4_RX0N                      |                                        |
    | A17/53                           |                       |            |              | MPQ3_RX2P                      |                                        |
    | A18/53                           |                       |            |              | MPQ3_RX2N                      |                                        |
    | A20/53                           |                       |            |              | MPQ3_RX0P                      |                                        |
    | A21/53                           |                       |            |              | MPQ3_RX0N                      |                                        |
    | A23/52                           |                       |            |              | MPQ2_RX2P                      |                                        |
    | A24/52                           |                       |            |              | MPQ2_RX2N                      |                                        |
    | A26/52                           |                       |            |              | MPQ2_RX0P                      |                                        |
    | A27/52                           |                       |            |              | MPQ2_RX0N                      |                                        |
    | A29/51                           |                       |            |              | MPQ1_RX2P                      |                                        |
    | A30/51                           |                       |            |              | MPQ1_RX2N                      |                                        |
    | A32/51                           |                       |            |              | MPQ1_RX0P                      |                                        |
    | A33/51                           |                       |            |              | MPQ1_RX0N                      |                                        |
    | AA1/3                            |     unused, PULL:DOWN |            |              | HPIO3_13B                      | PLLC3_IN                               |
    | AA2/3                            |     unused, PULL:DOWN |            |              | HPIO3_15A                      | DQ3_3                                  |
    | AA3/3                            |     unused, PULL:DOWN |            |              | HPIO3_17A                      | SD13_IN/DQ3_3                          |
    | AA4/3                            |     unused, PULL:DOWN |            |              | HPIO3_21A                      | SD17_IN/DQ3_3                          |
    | AA5/3                            |     unused, PULL:DOWN |            |              | HPIO3_23B                      | DQ3_3                                  |
    | AA7/3                            |     unused, PULL:DOWN |            |              | HPIO3_24B                      | PCLKRC3_2/PCLKEC3_2/ATB_TESTPAD2       |
    | AA8/3                            |     unused, PULL:DOWN |            |              | HPIO3_22A                      | DQ3_2                                  |
    | AA9/3                            |     unused, PULL:DOWN |            |              | HPIO3_22B                      | DQ3_2                                  |
    | AA10/3                           | Prohibited/Reserved   |            |              | HPIO3_12B                      | EXT_RES3                               |
    | AA11/3                           |     unused, PULL:DOWN |            |              | HPIO3_12A                      | VREF3                                  |
    | AA14/5                           |     unused, PULL:DOWN |            |              | HPIO5_0B                       | DQ5_0                                  |
    | AA15/5                           |     unused, PULL:DOWN |            |              | HPIO5_0A                       | DQ5_0                                  |
    | AA16/6                           |     unused, PULL:DOWN |            |              | HPIO6_0A                       | DQ6_0                                  |
    | AA17/6                           |     unused, PULL:DOWN |            |              | HPIO6_0B                       | DQ6_0                                  |
    | AA18/7                           |     unused, PULL:DOWN |            |              | HPIO7_0B                       | DQ7_0                                  |
    | AA19/8                           |     unused, PULL:DOWN |            |              | HPIO8_4B                       | DQSN8_0                                |
    | AA20/8                           |     unused, PULL:DOWN |            |              | HPIO8_2B                       | DQ8_0                                  |
    | AA21/10                          |     unused, PULL:DOWN |            |              | HPIO10_22B                     | DQ10_2                                 |
    | AA24/11                          |     unused, PULL:DOWN |            |              | HPIO11_16A                     | SD0_IN/DQ11_2                          |
    | AA26/11                          |     unused, PULL:DOWN |            |              | HPIO11_6A                      | HS11_PLL_MFGOUT1/DQ11_0                |
    | AA27/11                          |     unused, PULL:DOWN |            |              | HPIO11_0A                      | DQ11_0                                 |
    | AA28/11                          |     unused, PULL:DOWN |            |              | HPIO11_1B                      | DQ11_1                                 |
    | AA29/11                          |     unused, PULL:DOWN |            |              | HPIO11_25B                     | PCLKRC11_3/PCLKEC11_3                  |
    | AA30/11                          |     unused, PULL:DOWN |            |              | HPIO11_25A                     | PCLKRT11_3/PCLKET11_3/DM11_3           |
    | AA31/10                          |     unused, PULL:DOWN |            |              | HPIO10_7A                      | DQ10_1                                 |
    | AA32/10                          |     unused, PULL:DOWN |            |              | HPIO10_9A                      | DQ10_1                                 |
    | AA33/10                          |     unused, PULL:DOWN |            |              | HPIO10_11B                     | PCLKC10_1/PCLKRC10_1/PCLKEC10_1        |
    | AA34/10                          |     unused, PULL:DOWN |            |              | HPIO10_11A                     | PCLKT10_1/PCLKRT10_1/PCLKET10_1/DM10_1 |
    | AB1/3                            |     unused, PULL:DOWN |            |              | HPIO3_11A                      | PCLKT3_1/PCLKRT3_1/PCLKET3_1/DM3_1     |
    | AB4/3                            |     unused, PULL:DOWN |            |              | HPIO3_19A                      | SD15_IN/DQS3_3                         |
    | AB5/3                            |     unused, PULL:DOWN |            |              | HPIO3_19B                      | SD15_OUT/DQSN3_3                       |
    | AB7/3                            |     unused, PULL:DOWN |            |              | HPIO3_24A                      | PCLKRT3_2/PCLKET3_2/ATB_TESTPAD1/DM3_2 |
    | AB10/3                           |     unused, PULL:DOWN |            |              | HPIO3_20A                      | SD16_IN/DQ3_2                          |
    | AB12/3                           |     unused, PULL:DOWN |            |              | HPIO3_0B                       | DQ3_0                                  |
    | AB13/3                           |     unused, PULL:DOWN |            |              | HPIO3_0A                       | DQ3_0                                  |
    | AB14/5                           |     unused, PULL:DOWN |            |              | HPIO5_2A                       | DQ5_0                                  |
    | AB15/5                           |     unused, PULL:DOWN |            |              | HPIO5_2B                       | DQ5_0                                  |
    | AB16/6                           |     unused, PULL:DOWN |            |              | HPIO6_2A                       | DQ6_0                                  |
    | AB17/6                           |     unused, PULL:DOWN |            |              | HPIO6_2B                       | DQ6_0                                  |
    | AB18/7                           |     unused, PULL:DOWN |            |              | HPIO7_0A                       | DQ7_0                                  |
    | AB19/8                           |     unused, PULL:DOWN |            |              | HPIO8_4A                       | DQS8_0                                 |
    | AB20/8                           |     unused, PULL:DOWN |            |              | HPIO8_0B                       | DQ8_0                                  |
    | AB21/10                          |     unused, PULL:DOWN |            |              | HPIO10_24B                     | PCLKRC10_2/PCLKEC10_2                  |
    | AB24/10                          |     unused, PULL:DOWN |            |              | HPIO10_16B                     | SD2_OUT/DQ10_2                         |
    | AB25/10                          |     unused, PULL:DOWN |            |              | HPIO10_0A                      | DQ10_0                                 |
    | AB26/10                          |     unused, PULL:DOWN |            |              | HPIO10_2A                      | DQ10_0                                 |
    | AB27/10                          |     unused, PULL:DOWN |            |              | HPIO10_4A                      | DQS10_0                                |
    | AB28/10                          |     unused, PULL:DOWN |            |              | HPIO10_4B                      | DQSN10_0                               |
    | AB29/10                          |     unused, PULL:DOWN |            |              | HPIO10_6B                      | DQ10_0                                 |
    | AB30/10                          |     unused, PULL:DOWN |            |              | HPIO10_1A                      | DQ10_1                                 |
    | AB31/10                          |     unused, PULL:DOWN |            |              | HPIO10_7B                      | DQ10_1                                 |
    | AB32/10                          |     unused, PULL:DOWN |            |              | HPIO10_9B                      | DQ10_1                                 |
    | AB33/10                          |     unused, PULL:DOWN |            |              | HPIO10_17A                     | SD3_IN/DQ10_3                          |
    | AB34/10                          |     unused, PULL:DOWN |            |              | HPIO10_17B                     | SD3_OUT/DQ10_3                         |
    | AC1/3                            |     unused, PULL:DOWN |            |              | HPIO3_11B                      | PCLKC3_1/PCLKRC3_1/PCLKEC3_1           |
    | AC2/3                            |     unused, PULL:DOWN |            |              | HPIO3_7B                       | DQ3_1                                  |
    | AC3/3                            |     unused, PULL:DOWN |            |              | HPIO3_7A                       | DQ3_1                                  |
    | AC4/3                            |     unused, PULL:DOWN |            |              | HPIO3_5A                       | DQS3_1                                 |
    | AC5/3                            |     unused, PULL:DOWN |            |              | HPIO3_5B                       | DQSN3_1                                |
    | AC6/3                            |     unused, PULL:DOWN |            |              | HPIO3_18B                      | SD14_OUT/DQSN3_2                       |
    | AC7/3                            |     unused, PULL:DOWN |            |              | HPIO3_18A                      | SD14_IN/DQS3_2                         |
    | AC8/3                            |     unused, PULL:DOWN |            |              | HPIO3_10A                      | PCLKT3_0/PCLKRT3_0/PCLKET3_0/DM3_0     |
    | AC9/3                            |     unused, PULL:DOWN |            |              | HPIO3_10B                      | PCLKC3_0/PCLKRC3_0/PCLKEC3_0           |
    | AC10/3                           |     unused, PULL:DOWN |            |              | HPIO3_20B                      | SD16_OUT/DQ3_2                         |
    | AC12/3                           |     unused, PULL:DOWN |            |              | HPIO3_2B                       | DQ3_0                                  |
    | AC13/3                           |     unused, PULL:DOWN |            |              | HPIO3_2A                       | DQ3_0                                  |
    | AC14/5                           |     unused, PULL:DOWN |            |              | HPIO5_4B                       | DQSN5_0                                |
    | AC15/5                           |     unused, PULL:DOWN |            |              | HPIO5_4A                       | DQS5_0                                 |
    | AC16/6                           |     unused, PULL:DOWN |            |              | HPIO6_4B                       | DQSN6_0                                |
    | AC17/6                           |     unused, PULL:DOWN |            |              | HPIO6_4A                       | DQS6_0                                 |
    | AC20/8                           |     unused, PULL:DOWN |            |              | HPIO8_0A                       | DQ8_0                                  |
    | AC21/10                          |     unused, PULL:DOWN |            |              | HPIO10_24A                     | PCLKRT10_2/PCLKET10_2/DM10_2           |
    | AC23/10                          |     unused, PULL:DOWN |            |              | HPIO10_18A                     | DQS10_2                                |
    | AC24/10                          |     unused, PULL:DOWN |            |              | HPIO10_16A                     | SD2_IN/DQ10_2                          |
    | AC25/10                          |     unused, PULL:DOWN |            |              | HPIO10_0B                      | DQ10_0                                 |
    | AC26/10                          |     unused, PULL:DOWN |            |              | HPIO10_2B                      | DQ10_0                                 |
    | AC27/10                          |     unused, PULL:DOWN |            |              | HPIO10_8B                      | DQ10_0                                 |
    | AC29/10                          |     unused, PULL:DOWN |            |              | HPIO10_6A                      | HS10_PLL_MFGOUT1/DQ10_0                |
    | AC30/10                          |     unused, PULL:DOWN |            |              | HPIO10_1B                      | DQ10_1                                 |
    | AC33/10                          |     unused, PULL:DOWN |            |              | HPIO10_19B                     | DQSN10_3                               |
    | AC34/10                          |     unused, PULL:DOWN |            |              | HPIO10_19A                     | DQS10_3                                |
    | AD1/3                            |     unused, PULL:DOWN |            |              | HPIO3_9B                       | DQ3_1                                  |
    | AD2/3                            |     unused, PULL:DOWN |            |              | HPIO3_9A                       | DQ3_1                                  |
    | AD3/3                            |     unused, PULL:DOWN |            |              | HPIO3_3A                       | DQ3_1                                  |
    | AD4/3                            |     unused, PULL:DOWN |            |              | HPIO3_3B                       | DQ3_1                                  |
    | AD5/3                            |     unused, PULL:DOWN |            |              | HPIO3_1B                       | DQ3_1                                  |
    | AD6/3                            |     unused, PULL:DOWN |            |              | HPIO3_1A                       | DQ3_1                                  |
    | AD7/3                            |     unused, PULL:DOWN |            |              | HPIO3_8A                       | HS3_PLL_MFGOUT2/DQ3_0                  |
    | AD8/3                            |     unused, PULL:DOWN |            |              | HPIO3_8B                       | DQ3_0                                  |
    | AD9/3                            |     unused, PULL:DOWN |            |              | HPIO3_6A                       | HS3_PLL_MFGOUT1/DQ3_0                  |
    | AD10/3                           |     unused, PULL:DOWN |            |              | HPIO3_6B                       | DQ3_0                                  |
    | AD11/3                           |     unused, PULL:DOWN |            |              | HPIO3_4B                       | DQSN3_0                                |
    | AD12/3                           |     unused, PULL:DOWN |            |              | HPIO3_4A                       | DQS3_0                                 |
    | AD15/6                           |     unused, PULL:DOWN |            |              | HPIO6_24B                      | PCLKRC6_2/PCLKEC6_2                    |
    | AD17/7                           |     unused, PULL:DOWN |            |              | HPIO7_4A                       | DQS7_0                                 |
    | AD19/8                           |     unused, PULL:DOWN |            |              | HPIO8_6A                       | HS8_PLL_MFGOUT1/DQ8_0                  |
    | AD20/8                           |     unused, PULL:DOWN |            |              | HPIO8_6B                       | DQ8_0                                  |
    | AD21/10                          |     unused, PULL:DOWN |            |              | HPIO10_20A                     | DQ10_2                                 |
    | AD22/10                          |     unused, PULL:DOWN |            |              | HPIO10_20B                     | DQ10_2                                 |
    | AD23/10                          |     unused, PULL:DOWN |            |              | HPIO10_18B                     | DQSN10_2                               |
    | AD26/10                          |     unused, PULL:DOWN |            |              | HPIO10_10A                     | PCLKT10_0/PCLKRT10_0/PCLKET10_0/DM10_0 |
    | AD27/10                          |     unused, PULL:DOWN |            |              | HPIO10_8A                      | HS10_PLL_MFGOUT2/DQ10_0                |
    | AD29/10                          |     unused, PULL:DOWN |            |              | HPIO10_3B                      | DQ10_1                                 |
    | AD30/10                          |     unused, PULL:DOWN |            |              | HPIO10_3A                      | DQ10_1                                 |
    | AD31/10                          |     unused, PULL:DOWN |            |              | HPIO10_13B                     | PLLC10_IN                              |
    | AD32/10                          |     unused, PULL:DOWN |            |              | HPIO10_13A                     | PLLT10_IN                              |
    | AD33/10                          |     unused, PULL:DOWN |            |              | HPIO10_21A                     | DQ10_3                                 |
    | AD34/10                          |     unused, PULL:DOWN |            |              | HPIO10_21B                     | DQ10_3                                 |
    | AE1/4                            |     unused, PULL:DOWN |            |              | HPIO4_24B                      | PCLKRC4_2/PCLKEC4_2                    |
    | AE2/4                            |     unused, PULL:DOWN |            |              | HPIO4_20A                      | DQ4_2                                  |
    | AE3/4                            |     unused, PULL:DOWN |            |              | HPIO4_18B                      | DQSN4_2                                |
    | AE4/4                            |     unused, PULL:DOWN |            |              | HPIO4_16A                      | DQ4_2                                  |
    | AE5/4                            |     unused, PULL:DOWN |            |              | HPIO4_14A                      | DQ4_2                                  |
    | AE6/4                            |     unused, PULL:DOWN |            |              | HPIO4_10B                      | PCLKC4_0/PCLKRC4_0/PCLKEC4_0           |
    | AE7/4                            |     unused, PULL:DOWN |            |              | HPIO4_8A                       | HS4_PLL_MFGOUT2/DQ4_0                  |
    | AE9/4                            |     unused, PULL:DOWN |            |              | HPIO4_4B                       | DQSN4_0                                |
    | AE10/4                           |     unused, PULL:DOWN |            |              | HPIO4_2B                       | DQ4_0                                  |
    | AE11/4                           |     unused, PULL:DOWN |            |              | HPIO4_0A                       | DQ4_0                                  |
    | AE12/5                           |     unused, PULL:DOWN |            |              | HPIO5_24B                      | PCLKRC5_2/PCLKEC5_2                    |
    | AE13/5                           | Prohibited/Reserved   |            |              | HPIO5_12B                      | EXT_RES5                               |
    | AE14/5                           |     unused, PULL:DOWN |            |              | HPIO5_6A                       | HS5_PLL_MFGOUT1/DQ5_0                  |
    | AE15/6                           |     unused, PULL:DOWN |            |              | HPIO6_24A                      | PCLKRT6_2/PCLKET6_2/DM6_2              |
    | AE17/7                           |     unused, PULL:DOWN |            |              | HPIO7_4B                       | DQSN7_0                                |
    | AE18/7                           |     unused, PULL:DOWN |            |              | HPIO7_6A                       | HS7_PLL_MFGOUT1/DQ7_0                  |
    | AE19/7                           |     unused, PULL:DOWN |            |              | HPIO7_6B                       | DQ7_0                                  |
    | AE20/8                           |     unused, PULL:DOWN |            |              | HPIO8_8A                       | HS8_PLL_MFGOUT2/DQ8_0                  |
    | AE21/8                           |     unused, PULL:DOWN |            |              | HPIO8_8B                       | DQ8_0                                  |
    | AE22/8                           |     unused, PULL:DOWN |            |              | HPIO8_10A                      | PCLKT8_0/PCLKRT8_0/PCLKET8_0/DM8_0     |
    | AE23/8                           |     unused, PULL:DOWN |            |              | HPIO8_10B                      | PCLKC8_0/PCLKRC8_0/PCLKEC8_0           |
    | AE24/10                          |     unused, PULL:DOWN |            |              | HPIO10_14A                     | DQ10_2                                 |
    | AE25/10                          |     unused, PULL:DOWN |            |              | HPIO10_14B                     | DQ10_2                                 |
    | AE26/10                          |     unused, PULL:DOWN |            |              | HPIO10_10B                     | PCLKC10_0/PCLKRC10_0/PCLKEC10_0        |
    | AE27/10                          | Prohibited/Reserved   |            |              | HPIO10_12B                     | EXT_RES10                              |
    | AE28/10                          |     unused, PULL:DOWN |            |              | HPIO10_12A                     | VREF10                                 |
    | AE29/10                          |     unused, PULL:DOWN |            |              | HPIO10_5A                      | DQS10_1                                |
    | AE30/10                          |     unused, PULL:DOWN |            |              | HPIO10_5B                      | DQSN10_1                               |
    | AE31/10                          |     unused, PULL:DOWN |            |              | HPIO10_15A                     | DQ10_3                                 |
    | AE32/10                          |     unused, PULL:DOWN |            |              | HPIO10_15B                     | DQ10_3                                 |
    | AE33/10                          |     unused, PULL:DOWN |            |              | HPIO10_23B                     | DQ10_3                                 |
    | AE34/10                          |     unused, PULL:DOWN |            |              | HPIO10_23A                     | DQ10_3                                 |
    | AF1/4                            |     unused, PULL:DOWN |            |              | HPIO4_24A                      | PCLKRT4_2/PCLKET4_2/DM4_2              |
    | AF2/4                            |     unused, PULL:DOWN |            |              | HPIO4_20B                      | DQ4_2                                  |
    | AF3/4                            |     unused, PULL:DOWN |            |              | HPIO4_18A                      | DQS4_2                                 |
    | AF4/4                            |     unused, PULL:DOWN |            |              | HPIO4_16B                      | DQ4_2                                  |
    | AF5/4                            |     unused, PULL:DOWN |            |              | HPIO4_14B                      | DQ4_2                                  |
    | AF6/4                            |     unused, PULL:DOWN |            |              | HPIO4_10A                      | PCLKT4_0/PCLKRT4_0/PCLKET4_0/DM4_0     |
    | AF7/4                            |     unused, PULL:DOWN |            |              | HPIO4_8B                       | DQ4_0                                  |
    | AF9/4                            |     unused, PULL:DOWN |            |              | HPIO4_4A                       | DQS4_0                                 |
    | AF10/4                           |     unused, PULL:DOWN |            |              | HPIO4_2A                       | DQ4_0                                  |
    | AF11/4                           |     unused, PULL:DOWN |            |              | HPIO4_0B                       | DQ4_0                                  |
    | AF12/5                           |     unused, PULL:DOWN |            |              | HPIO5_24A                      | PCLKRT5_2/PCLKET5_2/DM5_2              |
    | AF13/5                           |     unused, PULL:DOWN |            |              | HPIO5_12A                      | VREF5                                  |
    | AF14/5                           |     unused, PULL:DOWN |            |              | HPIO5_6B                       | DQ5_0                                  |
    | AF15/6                           |     unused, PULL:DOWN |            |              | HPIO6_16A                      | DQ6_2                                  |
    | AF16/6                           |     unused, PULL:DOWN |            |              | HPIO6_16B                      | DQ6_2                                  |
    | AF17/7                           | Prohibited/Reserved   |            |              | HPIO7_12B                      | EXT_RES7                               |
    | AF18/7                           |     unused, PULL:DOWN |            |              | HPIO7_12A                      | VREF7                                  |
    | AF19/7                           |     unused, PULL:DOWN |            |              | HPIO7_8A                       | HS7_PLL_MFGOUT2/DQ7_0                  |
    | AF20/7                           |     unused, PULL:DOWN |            |              | HPIO7_8B                       | DQ7_0                                  |
    | AF21/8                           |     unused, PULL:DOWN |            |              | HPIO8_18A                      | SD8_IN/DQS8_2                          |
    | AF23/8                           | Prohibited/Reserved   |            |              | HPIO8_12B                      | EXT_RES8                               |
    | AF24/8                           |     unused, PULL:DOWN |            |              | HPIO8_12A                      | VREF8                                  |
    | AF25/8                           |     unused, PULL:DOWN |            |              | HPIO8_14B                      | DQ8_2                                  |
    | AF26/9                           | Prohibited/Reserved   |            |              | HPIO9_12B                      | EXT_RES9                               |
    | AF27/9                           |     unused, PULL:DOWN |            |              | HPIO9_12A                      | VREF9                                  |
    | AF28/9                           |     unused, PULL:DOWN |            |              | HPIO9_0A                       | DQ9_0                                  |
    | AF29/9                           |     unused, PULL:DOWN |            |              | HPIO9_0B                       | DQ9_0                                  |
    | AF30/9                           |     unused, PULL:DOWN |            |              | HPIO9_2A                       | DQ9_0                                  |
    | AF31/9                           |     unused, PULL:DOWN |            |              | HPIO9_4A                       | DQS9_0                                 |
    | AF32/9                           |     unused, PULL:DOWN |            |              | HPIO9_6B                       | DQ9_0                                  |
    | AF33/10                          |     unused, PULL:DOWN |            |              | HPIO10_25A                     | PCLKRT10_3/PCLKET10_3/DM10_3           |
    | AF34/10                          |     unused, PULL:DOWN |            |              | HPIO10_25B                     | PCLKRC10_3/PCLKEC10_3                  |
    | AG1/4                            |     unused, PULL:DOWN |            |              | HPIO4_22A                      | DQ4_2                                  |
    | AG2/4                            |     unused, PULL:DOWN |            |              | HPIO4_22B                      | DQ4_2                                  |
    | AG5/4                            | Prohibited/Reserved   |            |              | HPIO4_12B                      | EXT_RES4                               |
    | AG6/4                            |     unused, PULL:DOWN |            |              | HPIO4_12A                      | VREF4                                  |
    | AG7/4                            |     unused, PULL:DOWN |            |              | HPIO4_6A                       | HS4_PLL_MFGOUT1/DQ4_0                  |
    | AG8/4                            |     unused, PULL:DOWN |            |              | HPIO4_6B                       | DQ4_0                                  |
    | AG9/5                            |     unused, PULL:DOWN |            |              | HPIO5_18B                      | DQSN5_2                                |
    | AG10/5                           |     unused, PULL:DOWN |            |              | HPIO5_20A                      | DQ5_2                                  |
    | AG11/5                           |     unused, PULL:DOWN |            |              | HPIO5_20B                      | DQ5_2                                  |
    | AG12/5                           |     unused, PULL:DOWN |            |              | HPIO5_8A                       | HS5_PLL_MFGOUT2/DQ5_0                  |
    | AG13/5                           |     unused, PULL:DOWN |            |              | HPIO5_8B                       | DQ5_0                                  |
    | AG14/6                           |     unused, PULL:DOWN |            |              | HPIO6_18B                      | DQSN6_2                                |
    | AG15/6                           |     unused, PULL:DOWN |            |              | HPIO6_14A                      | DQ6_2                                  |
    | AG16/6                           |     unused, PULL:DOWN |            |              | HPIO6_10B                      | PCLKC6_0/PCLKRC6_0/PCLKEC6_0           |
    | AG17/6                           |     unused, PULL:DOWN |            |              | HPIO6_6B                       | DQ6_0                                  |
    | AG18/7                           |     unused, PULL:DOWN |            |              | HPIO7_16B                      | DQ7_2                                  |
    | AG20/7                           |     unused, PULL:DOWN |            |              | HPIO7_10A                      | PCLKT7_0/PCLKRT7_0/PCLKET7_0/DM7_0     |
    | AG21/8                           |     unused, PULL:DOWN |            |              | HPIO8_18B                      | SD8_OUT/DQSN8_2                        |
    | AG23/8                           |     unused, PULL:DOWN |            |              | HPIO8_16A                      | SD6_IN/DQ8_2                           |
    | AG24/8                           |     unused, PULL:DOWN |            |              | HPIO8_16B                      | SD6_OUT/DQ8_2                          |
    | AG25/8                           |     unused, PULL:DOWN |            |              | HPIO8_14A                      | DQ8_2                                  |
    | AG26/9                           |     unused, PULL:DOWN |            |              | HPIO9_22B                      | DQ9_2                                  |
    | AG27/9                           |     unused, PULL:DOWN |            |              | HPIO9_14A                      | DQ9_2                                  |
    | AG28/9                           |     unused, PULL:DOWN |            |              | HPIO9_14B                      | DQ9_2                                  |
    | AG29/9                           |     unused, PULL:DOWN |            |              | HPIO9_16B                      | SD4_OUT/DQ9_2                          |
    | AG30/9                           |     unused, PULL:DOWN |            |              | HPIO9_2B                       | DQ9_0                                  |
    | AG31/9                           |     unused, PULL:DOWN |            |              | HPIO9_4B                       | DQSN9_0                                |
    | AG32/9                           |     unused, PULL:DOWN |            |              | HPIO9_6A                       | HS9_PLL_MFGOUT1/DQ9_0                  |
    | AG33/9                           |     unused, PULL:DOWN |            |              | HPIO9_10A                      | PCLKT9_0/PCLKRT9_0/PCLKET9_0/DM9_0     |
    | AG34/9                           |     unused, PULL:DOWN |            |              | HPIO9_8B                       | DQ9_0                                  |
    | AH1/4                            |     unused, PULL:DOWN |            |              | HPIO4_25A                      | PCLKRT4_3/PCLKET4_3/DM4_3              |
    | AH2/4                            |     unused, PULL:DOWN |            |              | HPIO4_23A                      | DQ4_3                                  |
    | AH3/4                            |     unused, PULL:DOWN |            |              | HPIO4_21B                      | DQ4_3                                  |
    | AH4/4                            |     unused, PULL:DOWN |            |              | HPIO4_21A                      | DQ4_3                                  |
    | AH5/4                            |     unused, PULL:DOWN |            |              | HPIO4_1B                       | DQ4_1                                  |
    | AH6/4                            |     unused, PULL:DOWN |            |              | HPIO4_1A                       | DQ4_1                                  |
    | AH7/5                            |     unused, PULL:DOWN |            |              | HPIO5_22A                      | DQ5_2                                  |
    | AH8/5                            |     unused, PULL:DOWN |            |              | HPIO5_22B                      | DQ5_2                                  |
    | AH9/5                            |     unused, PULL:DOWN |            |              | HPIO5_18A                      | DQS5_2                                 |
    | AH10/5                           |     unused, PULL:DOWN |            |              | HPIO5_16A                      | DQ5_2                                  |
    | AH13/6                           |     unused, PULL:DOWN |            |              | HPIO6_22A                      | DQ6_2                                  |
    | AH14/6                           |     unused, PULL:DOWN |            |              | HPIO6_18A                      | DQS6_2                                 |
    | AH15/6                           |     unused, PULL:DOWN |            |              | HPIO6_14B                      | DQ6_2                                  |
    | AH16/6                           |     unused, PULL:DOWN |            |              | HPIO6_10A                      | PCLKT6_0/PCLKRT6_0/PCLKET6_0/DM6_0     |
    | AH17/6                           |     unused, PULL:DOWN |            |              | HPIO6_6A                       | HS6_PLL_MFGOUT1/DQ6_0                  |
    | AH18/7                           |     unused, PULL:DOWN |            |              | HPIO7_16A                      | DQ7_2                                  |
    | AH20/7                           |     unused, PULL:DOWN |            |              | HPIO7_10B                      | PCLKC7_0/PCLKRC7_0/PCLKEC7_0           |
    | AH21/7                           |     unused, PULL:DOWN |            |              | HPIO7_14A                      | DQ7_2                                  |
    | AH22/7                           |     unused, PULL:DOWN |            |              | HPIO7_14B                      | DQ7_2                                  |
    | AH23/8                           |     unused, PULL:DOWN |            |              | HPIO8_22B                      | DQ8_2                                  |
    | AH24/8                           |     unused, PULL:DOWN |            |              | HPIO8_20A                      | SD10_IN/DQ8_2                          |
    | AH25/8                           |     unused, PULL:DOWN |            |              | HPIO8_20B                      | SD10_OUT/DQ8_2                         |
    | AH26/9                           |     unused, PULL:DOWN |            |              | HPIO9_22A                      | DQ9_2                                  |
    | AH29/9                           |     unused, PULL:DOWN |            |              | HPIO9_16A                      | SD4_IN/DQ9_2                           |
    | AH30/9                           |     unused, PULL:DOWN |            |              | HPIO9_18A                      | DQS9_2                                 |
    | AH33/9                           |     unused, PULL:DOWN |            |              | HPIO9_10B                      | PCLKC9_0/PCLKRC9_0/PCLKEC9_0           |
    | AH34/9                           |     unused, PULL:DOWN |            |              | HPIO9_8A                       | HS9_PLL_MFGOUT2/DQ9_0                  |
    | AJ1/4                            |     unused, PULL:DOWN |            |              | HPIO4_25B                      | PCLKRC4_3/PCLKEC4_3                    |
    | AJ2/4                            |     unused, PULL:DOWN |            |              | HPIO4_19A                      | DQS4_3                                 |
    | AJ3/4                            |     unused, PULL:DOWN |            |              | HPIO4_23B                      | DQ4_3                                  |
    | AJ4/4                            |     unused, PULL:DOWN |            |              | HPIO4_3A                       | DQ4_1                                  |
    | AJ5/5                            |     unused, PULL:DOWN |            |              | HPIO5_25A                      | PCLKRT5_3/PCLKET5_3/DM5_3              |
    | AJ6/5                            |     unused, PULL:DOWN |            |              | HPIO5_25B                      | PCLKRC5_3/PCLKEC5_3                    |
    | AJ7/5                            |     unused, PULL:DOWN |            |              | HPIO5_21B                      | DQ5_3                                  |
    | AJ10/5                           |     unused, PULL:DOWN |            |              | HPIO5_16B                      | DQ5_2                                  |
    | AJ11/5                           |     unused, PULL:DOWN |            |              | HPIO5_10B                      | PCLKC5_0/PCLKRC5_0/PCLKEC5_0           |
    | AJ12/5                           |     unused, PULL:DOWN |            |              | HPIO5_10A                      | PCLKT5_0/PCLKRT5_0/PCLKET5_0/DM5_0     |
    | AJ13/6                           |     unused, PULL:DOWN |            |              | HPIO6_22B                      | DQ6_2                                  |
    | AJ16/6                           |     unused, PULL:DOWN |            |              | HPIO6_12A                      | VREF6                                  |
    | AJ17/6                           |     unused, PULL:DOWN |            |              | HPIO6_8B                       | DQ6_0                                  |
    | AJ18/7                           |     unused, PULL:DOWN |            |              | HPIO7_24A                      | PCLKRT7_2/PCLKET7_2/DM7_2              |
    | AJ19/7                           |     unused, PULL:DOWN |            |              | HPIO7_22B                      | DQ7_2                                  |
    | AJ20/7                           |     unused, PULL:DOWN |            |              | HPIO7_20B                      | DQ7_2                                  |
    | AJ21/7                           |     unused, PULL:DOWN |            |              | HPIO7_18B                      | DQSN7_2                                |
    | AJ22/7                           |     unused, PULL:DOWN |            |              | HPIO7_18A                      | DQS7_2                                 |
    | AJ23/8                           |     unused, PULL:DOWN |            |              | HPIO8_22A                      | DQ8_2                                  |
    | AJ26/9                           |     unused, PULL:DOWN |            |              | HPIO9_24B                      | PCLKRC9_2/PCLKEC9_2                    |
    | AJ27/9                           |     unused, PULL:DOWN |            |              | HPIO9_24A                      | PCLKRT9_2/PCLKET9_2/DM9_2              |
    | AJ28/9                           |     unused, PULL:DOWN |            |              | HPIO9_20A                      | DQ9_2                                  |
    | AJ29/9                           |     unused, PULL:DOWN |            |              | HPIO9_20B                      | DQ9_2                                  |
    | AJ30/9                           |     unused, PULL:DOWN |            |              | HPIO9_18B                      | DQSN9_2                                |
    | AJ31/9                           |     unused, PULL:DOWN |            |              | HPIO9_1A                       | DQ9_1                                  |
    | AJ32/9                           |     unused, PULL:DOWN |            |              | HPIO9_1B                       | DQ9_1                                  |
    | AJ33/9                           |     unused, PULL:DOWN |            |              | HPIO9_3B                       | DQ9_1                                  |
    | AJ34/9                           |     unused, PULL:DOWN |            |              | HPIO9_3A                       | DQ9_1                                  |
    | AK1/4                            |     unused, PULL:DOWN |            |              | HPIO4_17B                      | DQ4_3                                  |
    | AK2/4                            |     unused, PULL:DOWN |            |              | HPIO4_19B                      | DQSN4_3                                |
    | AK4/4                            |     unused, PULL:DOWN |            |              | HPIO4_3B                       | DQ4_1                                  |
    | AK5/5                            |     unused, PULL:DOWN |            |              | HPIO5_23A                      | DQ5_3                                  |
    | AK6/5                            |     unused, PULL:DOWN |            |              | HPIO5_23B                      | DQ5_3                                  |
    | AK7/5                            |     unused, PULL:DOWN |            |              | HPIO5_21A                      | DQ5_3                                  |
    | AK8/5                            |     unused, PULL:DOWN |            |              | HPIO5_1B                       | DQ5_1                                  |
    | AK9/5                            |     unused, PULL:DOWN |            |              | HPIO5_1A                       | DQ5_1                                  |
    | AK10/5                           |     unused, PULL:DOWN |            |              | HPIO5_14A                      | DQ5_2                                  |
    | AK11/5                           |     unused, PULL:DOWN |            |              | HPIO5_14B                      | DQ5_2                                  |
    | AK12/6                           |     unused, PULL:DOWN |            |              | HPIO6_15B                      | DQ6_3                                  |
    | AK13/6                           |     unused, PULL:DOWN |            |              | HPIO6_15A                      | DQ6_3                                  |
    | AK14/6                           |     unused, PULL:DOWN |            |              | HPIO6_20A                      | DQ6_2                                  |
    | AK15/6                           |     unused, PULL:DOWN |            |              | HPIO6_20B                      | DQ6_2                                  |
    | AK16/6                           | Prohibited/Reserved   |            |              | HPIO6_12B                      | EXT_RES6                               |
    | AK17/6                           |     unused, PULL:DOWN |            |              | HPIO6_8A                       | HS6_PLL_MFGOUT2/DQ6_0                  |
    | AK18/7                           |     unused, PULL:DOWN |            |              | HPIO7_24B                      | PCLKRC7_2/PCLKEC7_2                    |
    | AK19/7                           |     unused, PULL:DOWN |            |              | HPIO7_22A                      | DQ7_2                                  |
    | AK20/7                           |     unused, PULL:DOWN |            |              | HPIO7_20A                      | DQ7_2                                  |
    | AK21/7                           |     unused, PULL:DOWN |            |              | HPIO7_1A                       | DQ7_1                                  |
    | AK22/7                           |     unused, PULL:DOWN |            |              | HPIO7_1B                       | DQ7_1                                  |
    | AK23/8                           |     unused, PULL:DOWN |            |              | HPIO8_24B                      | PCLKRC8_2/PCLKEC8_2                    |
    | AK24/8                           |     unused, PULL:DOWN |            |              | HPIO8_24A                      | PCLKRT8_2/PCLKET8_2/DM8_2              |
    | AK25/8                           |     unused, PULL:DOWN |            |              | HPIO8_1A                       | DQ8_1                                  |
    | AK26/8                           |     unused, PULL:DOWN |            |              | HPIO8_3B                       | DQ8_1                                  |
    | AK27/8                           |     unused, PULL:DOWN |            |              | HPIO8_5B                       | DQSN8_1                                |
    | AK28/8                           |     unused, PULL:DOWN |            |              | HPIO8_5A                       | DQS8_1                                 |
    | AK29/9                           |     unused, PULL:DOWN |            |              | HPIO9_5A                       | DQS9_1                                 |
    | AK30/9                           |     unused, PULL:DOWN |            |              | HPIO9_5B                       | DQSN9_1                                |
    | AK31/9                           |     unused, PULL:DOWN |            |              | HPIO9_7A                       | DQ9_1                                  |
    | AK32/9                           |     unused, PULL:DOWN |            |              | HPIO9_7B                       | DQ9_1                                  |
    | AK33/9                           |     unused, PULL:DOWN |            |              | HPIO9_9A                       | DQ9_1                                  |
    | AK34/9                           |     unused, PULL:DOWN |            |              | HPIO9_9B                       | DQ9_1                                  |
    | AL1/4                            |     unused, PULL:DOWN |            |              | HPIO4_17A                      | DQ4_3                                  |
    | AL2/4                            |     unused, PULL:DOWN |            |              | HPIO4_13A                      | PLLT4_IN                               |
    | AL4/4                            |     unused, PULL:DOWN |            |              | HPIO4_5B                       | DQSN4_1                                |
    | AL5/5                            |     unused, PULL:DOWN |            |              | HPIO5_19A                      | DQS5_3                                 |
    | AL6/5                            |     unused, PULL:DOWN |            |              | HPIO5_19B                      | DQSN5_3                                |
    | AL8/5                            |     unused, PULL:DOWN |            |              | HPIO5_3A                       | DQ5_1                                  |
    | AL9/5                            |     unused, PULL:DOWN |            |              | HPIO5_3B                       | DQ5_1                                  |
    | AL10/6                           |     unused, PULL:DOWN |            |              | HPIO6_25A                      | PCLKRT6_3/PCLKET6_3/DM6_3              |
    | AL11/6                           |     unused, PULL:DOWN |            |              | HPIO6_25B                      | PCLKRC6_3/PCLKEC6_3                    |
    | AL13/6                           |     unused, PULL:DOWN |            |              | HPIO6_13A                      | PLLT6_IN                               |
    | AL14/6                           |     unused, PULL:DOWN |            |              | HPIO6_7B                       | DQ6_1                                  |
    | AL16/6                           |     unused, PULL:DOWN |            |              | HPIO6_1A                       | DQ6_1                                  |
    | AL17/7                           |     unused, PULL:DOWN |            |              | HPIO7_23B                      | DQ7_3                                  |
    | AL18/7                           |     unused, PULL:DOWN |            |              | HPIO7_19B                      | DQSN7_3                                |
    | AL20/7                           |     unused, PULL:DOWN |            |              | HPIO7_7A                       | DQ7_1                                  |
    | AL21/7                           |     unused, PULL:DOWN |            |              | HPIO7_5B                       | DQSN7_1                                |
    | AL23/7                           |     unused, PULL:DOWN |            |              | HPIO7_3B                       | DQ7_1                                  |
    | AL24/8                           |     unused, PULL:DOWN |            |              | HPIO8_25B                      | PCLKRC8_3/PCLKEC8_3                    |
    | AL25/8                           |     unused, PULL:DOWN |            |              | HPIO8_1B                       | DQ8_1                                  |
    | AL26/8                           |     unused, PULL:DOWN |            |              | HPIO8_3A                       | DQ8_1                                  |
    | AL27/8                           |     unused, PULL:DOWN |            |              | HPIO8_7A                       | DQ8_1                                  |
    | AL28/8                           |     unused, PULL:DOWN |            |              | HPIO8_7B                       | DQ8_1                                  |
    | AL29/8                           |     unused, PULL:DOWN |            |              | HPIO8_9A                       | DQ8_1                                  |
    | AL30/9                           |     unused, PULL:DOWN |            |              | HPIO9_11B                      | PCLKC9_1/PCLKRC9_1/PCLKEC9_1           |
    | AL33/9                           |     unused, PULL:DOWN |            |              | HPIO9_15A                      | DQ9_3                                  |
    | AL34/9                           |     unused, PULL:DOWN |            |              | HPIO9_15B                      | DQ9_3                                  |
    | AM1/4                            |     unused, PULL:DOWN |            |              | HPIO4_15B                      | DQ4_3                                  |
    | AM2/4                            |     unused, PULL:DOWN |            |              | HPIO4_13B                      | PLLC4_IN                               |
    | AM3/4                            |     unused, PULL:DOWN |            |              | HPIO4_9A                       | DQ4_1                                  |
    | AM4/4                            |     unused, PULL:DOWN |            |              | HPIO4_5A                       | DQS4_1                                 |
    | AM5/5                            |     unused, PULL:DOWN |            |              | HPIO5_17B                      | DQ5_3                                  |
    | AM6/5                            |     unused, PULL:DOWN |            |              | HPIO5_17A                      | DQ5_3                                  |
    | AM8/5                            |     unused, PULL:DOWN |            |              | HPIO5_5A                       | DQS5_1                                 |
    | AM9/5                            |     unused, PULL:DOWN |            |              | HPIO5_5B                       | DQSN5_1                                |
    | AM10/6                           |     unused, PULL:DOWN |            |              | HPIO6_23A                      | DQ6_3                                  |
    | AM11/6                           |     unused, PULL:DOWN |            |              | HPIO6_23B                      | DQ6_3                                  |
    | AM13/6                           |     unused, PULL:DOWN |            |              | HPIO6_13B                      | PLLC6_IN                               |
    | AM14/6                           |     unused, PULL:DOWN |            |              | HPIO6_7A                       | DQ6_1                                  |
    | AM16/6                           |     unused, PULL:DOWN |            |              | HPIO6_1B                       | DQ6_1                                  |
    | AM17/7                           |     unused, PULL:DOWN |            |              | HPIO7_23A                      | DQ7_3                                  |
    | AM18/7                           |     unused, PULL:DOWN |            |              | HPIO7_19A                      | DQS7_3                                 |
    | AM20/7                           |     unused, PULL:DOWN |            |              | HPIO7_7B                       | DQ7_1                                  |
    | AM21/7                           |     unused, PULL:DOWN |            |              | HPIO7_5A                       | DQS7_1                                 |
    | AM23/7                           |     unused, PULL:DOWN |            |              | HPIO7_3A                       | DQ7_1                                  |
    | AM24/8                           |     unused, PULL:DOWN |            |              | HPIO8_25A                      | PCLKRT8_3/PCLKET8_3/DM8_3              |
    | AM25/8                           |     unused, PULL:DOWN |            |              | HPIO8_17B                      | SD7_OUT/DQ8_3                          |
    | AM26/8                           |     unused, PULL:DOWN |            |              | HPIO8_17A                      | SD7_IN/DQ8_3                           |
    | AM28/8                           |     unused, PULL:DOWN |            |              | HPIO8_11B                      | PCLKC8_1/PCLKRC8_1/PCLKEC8_1           |
    | AM29/8                           |     unused, PULL:DOWN |            |              | HPIO8_9B                       | DQ8_1                                  |
    | AM30/9                           |     unused, PULL:DOWN |            |              | HPIO9_11A                      | PCLKT9_1/PCLKRT9_1/PCLKET9_1/DM9_1     |
    | AM31/9                           |     unused, PULL:DOWN |            |              | HPIO9_13B                      | PLLC9_IN                               |
    | AM32/9                           |     unused, PULL:DOWN |            |              | HPIO9_13A                      | PLLT9_IN                               |
    | AM33/9                           |     unused, PULL:DOWN |            |              | HPIO9_17A                      | SD5_IN/DQ9_3                           |
    | AM34/9                           |     unused, PULL:DOWN |            |              | HPIO9_17B                      | SD5_OUT/DQ9_3                          |
    | AN1/4                            |     unused, PULL:DOWN |            |              | HPIO4_15A                      | DQ4_3                                  |
    | AN3/4                            |     unused, PULL:DOWN |            |              | HPIO4_9B                       | DQ4_1                                  |
    | AN4/4                            |     unused, PULL:DOWN |            |              | HPIO4_7A                       | DQ4_1                                  |
    | AN5/5                            |     unused, PULL:DOWN |            |              | HPIO5_15B                      | DQ5_3                                  |
    | AN6/5                            |     unused, PULL:DOWN |            |              | HPIO5_15A                      | DQ5_3                                  |
    | AN7/5                            |     unused, PULL:DOWN |            |              | HPIO5_11A                      | PCLKT5_1/PCLKRT5_1/PCLKET5_1/DM5_1     |
    | AN8/5                            |     unused, PULL:DOWN |            |              | HPIO5_7B                       | DQ5_1                                  |
    | AN9/5                            |     unused, PULL:DOWN |            |              | HPIO5_7A                       | DQ5_1                                  |
    | AN10/6                           |     unused, PULL:DOWN |            |              | HPIO6_21B                      | DQ6_3                                  |
    | AN11/6                           |     unused, PULL:DOWN |            |              | HPIO6_21A                      | DQ6_3                                  |
    | AN12/6                           |     unused, PULL:DOWN |            |              | HPIO6_17B                      | DQ6_3                                  |
    | AN13/6                           |     unused, PULL:DOWN |            |              | HPIO6_11A                      | PCLKT6_1/PCLKRT6_1/PCLKET6_1/DM6_1     |
    | AN14/6                           |     unused, PULL:DOWN |            |              | HPIO6_9A                       | DQ6_1                                  |
    | AN15/6                           |     unused, PULL:DOWN |            |              | HPIO6_5B                       | DQSN6_1                                |
    | AN16/6                           |     unused, PULL:DOWN |            |              | HPIO6_3B                       | DQ6_1                                  |
    | AN17/7                           |     unused, PULL:DOWN |            |              | HPIO7_25B                      | PCLKRC7_3/PCLKEC7_3                    |
    | AN18/7                           |     unused, PULL:DOWN |            |              | HPIO7_21A                      | DQ7_3                                  |
    | AN19/7                           |     unused, PULL:DOWN |            |              | HPIO7_17A                      | DQ7_3                                  |
    | AN20/7                           |     unused, PULL:DOWN |            |              | HPIO7_15A                      | DQ7_3                                  |
    | AN21/7                           |     unused, PULL:DOWN |            |              | HPIO7_13B                      | PLLC7_IN                               |
    | AN22/7                           |     unused, PULL:DOWN |            |              | HPIO7_11B                      | PCLKC7_1/PCLKRC7_1/PCLKEC7_1           |
    | AN23/7                           |     unused, PULL:DOWN |            |              | HPIO7_9A                       | DQ7_1                                  |
    | AN24/8                           |     unused, PULL:DOWN |            |              | HPIO8_23A                      | DQ8_3                                  |
    | AN25/8                           |     unused, PULL:DOWN |            |              | HPIO8_21A                      | SD11_IN/DQ8_3                          |
    | AN26/8                           |     unused, PULL:DOWN |            |              | HPIO8_19B                      | SD9_OUT/DQSN8_3                        |
    | AN28/8                           |     unused, PULL:DOWN |            |              | HPIO8_11A                      | PCLKT8_1/PCLKRT8_1/PCLKET8_1/DM8_1     |
    | AN29/8                           |     unused, PULL:DOWN |            |              | HPIO8_13B                      | PLLC8_IN                               |
    | AN30/9                           |     unused, PULL:DOWN |            |              | HPIO9_25B                      | PCLKRC9_3/PCLKEC9_3                    |
    | AN31/9                           |     unused, PULL:DOWN |            |              | HPIO9_23B                      | DQ9_3                                  |
    | AN32/9                           |     unused, PULL:DOWN |            |              | HPIO9_21A                      | DQ9_3                                  |
    | AN33/9                           |     unused, PULL:DOWN |            |              | HPIO9_19B                      | DQSN9_3                                |
    | AN34/9                           |     unused, PULL:DOWN |            |              | HPIO9_19A                      | DQS9_3                                 |
    | AP2/4                            |     unused, PULL:DOWN |            |              | HPIO4_11A                      | PCLKT4_1/PCLKRT4_1/PCLKET4_1/DM4_1     |
    | AP3/4                            |     unused, PULL:DOWN |            |              | HPIO4_11B                      | PCLKC4_1/PCLKRC4_1/PCLKEC4_1           |
    | AP4/4                            |     unused, PULL:DOWN |            |              | HPIO4_7B                       | DQ4_1                                  |
    | AP5/5                            |     unused, PULL:DOWN |            |              | HPIO5_13A                      | PLLT5_IN                               |
    | AP6/5                            |     unused, PULL:DOWN |            |              | HPIO5_13B                      | PLLC5_IN                               |
    | AP7/5                            |     unused, PULL:DOWN |            |              | HPIO5_11B                      | PCLKC5_1/PCLKRC5_1/PCLKEC5_1           |
    | AP8/5                            |     unused, PULL:DOWN |            |              | HPIO5_9B                       | DQ5_1                                  |
    | AP9/5                            |     unused, PULL:DOWN |            |              | HPIO5_9A                       | DQ5_1                                  |
    | AP10/6                           |     unused, PULL:DOWN |            |              | HPIO6_19A                      | DQS6_3                                 |
    | AP11/6                           |     unused, PULL:DOWN |            |              | HPIO6_19B                      | DQSN6_3                                |
    | AP12/6                           |     unused, PULL:DOWN |            |              | HPIO6_17A                      | DQ6_3                                  |
    | AP13/6                           |     unused, PULL:DOWN |            |              | HPIO6_11B                      | PCLKC6_1/PCLKRC6_1/PCLKEC6_1           |
    | AP14/6                           |     unused, PULL:DOWN |            |              | HPIO6_9B                       | DQ6_1                                  |
    | AP15/6                           |     unused, PULL:DOWN |            |              | HPIO6_5A                       | DQS6_1                                 |
    | AP16/6                           |     unused, PULL:DOWN |            |              | HPIO6_3A                       | DQ6_1                                  |
    | AP17/7                           |     unused, PULL:DOWN |            |              | HPIO7_25A                      | PCLKRT7_3/PCLKET7_3/DM7_3              |
    | AP18/7                           |     unused, PULL:DOWN |            |              | HPIO7_21B                      | DQ7_3                                  |
    | AP19/7                           |     unused, PULL:DOWN |            |              | HPIO7_17B                      | DQ7_3                                  |
    | AP20/7                           |     unused, PULL:DOWN |            |              | HPIO7_15B                      | DQ7_3                                  |
    | AP21/7                           |     unused, PULL:DOWN |            |              | HPIO7_13A                      | PLLT7_IN                               |
    | AP22/7                           |     unused, PULL:DOWN |            |              | HPIO7_11A                      | PCLKT7_1/PCLKRT7_1/PCLKET7_1/DM7_1     |
    | AP23/7                           |     unused, PULL:DOWN |            |              | HPIO7_9B                       | DQ7_1                                  |
    | AP24/8                           |     unused, PULL:DOWN |            |              | HPIO8_23B                      | DQ8_3                                  |
    | AP25/8                           |     unused, PULL:DOWN |            |              | HPIO8_21B                      | SD11_OUT/DQ8_3                         |
    | AP26/8                           |     unused, PULL:DOWN |            |              | HPIO8_19A                      | SD9_IN/DQS8_3                          |
    | AP27/8                           |     unused, PULL:DOWN |            |              | HPIO8_15B                      | DQ8_3                                  |
    | AP28/8                           |     unused, PULL:DOWN |            |              | HPIO8_15A                      | DQ8_3                                  |
    | AP29/8                           |     unused, PULL:DOWN |            |              | HPIO8_13A                      | PLLT8_IN                               |
    | AP30/9                           |     unused, PULL:DOWN |            |              | HPIO9_25A                      | PCLKRT9_3/PCLKET9_3/DM9_3              |
    | AP31/9                           |     unused, PULL:DOWN |            |              | HPIO9_23A                      | DQ9_3                                  |
    | AP32/9                           |     unused, PULL:DOWN |            |              | HPIO9_21B                      | DQ9_3                                  |
    | B1/56                            |                       |            |              | MPQ6_RX0N                      |                                        |
    | B3/56                            |                       |            |              | MPQ6_RX1N                      |                                        |
    | C1/56                            |                       |            |              | MPQ6_RX0P                      |                                        |
    | C3/56                            |                       |            |              | MPQ6_RX1P                      |                                        |
    | C5/55                            |                       |            |              | MPQ5_RX3P                      |                                        |
    | C6/55                            |                       |            |              | MPQ5_RX3N                      |                                        |
    | C8/55                            |                       |            |              | MPQ5_RX1P                      |                                        |
    | C9/55                            |                       |            |              | MPQ5_RX1N                      |                                        |
    | C11/54                           |                       |            |              | MPQ4_RX3P                      |                                        |
    | C12/54                           |                       |            |              | MPQ4_RX3N                      |                                        |
    | C14/54                           |                       |            |              | MPQ4_RX1P                      |                                        |
    | C15/54                           |                       |            |              | MPQ4_RX1N                      |                                        |
    | C17/53                           |                       |            |              | MPQ3_RX3P                      |                                        |
    | C18/53                           |                       |            |              | MPQ3_RX3N                      |                                        |
    | C20/53                           |                       |            |              | MPQ3_RX1P                      |                                        |
    | C21/53                           |                       |            |              | MPQ3_RX1N                      |                                        |
    | C23/52                           |                       |            |              | MPQ2_RX3P                      |                                        |
    | C24/52                           |                       |            |              | MPQ2_RX3N                      |                                        |
    | C26/52                           |                       |            |              | MPQ2_RX1P                      |                                        |
    | C27/52                           |                       |            |              | MPQ2_RX1N                      |                                        |
    | C29/51                           |                       |            |              | MPQ1_RX3P                      |                                        |
    | C30/51                           |                       |            |              | MPQ1_RX3N                      |                                        |
    | C32/51                           |                       |            |              | MPQ1_RX1P                      |                                        |
    | C33/51                           |                       |            |              | MPQ1_RX1N                      |                                        |
    | E1/56                            |                       |            |              | MPQ6_RX2N                      |                                        |
    | E3/56                            |                       |            |              | MPQ6_RX3N                      |                                        |
    | E5/55                            |                       |            |              | MPQ5_TX2P                      |                                        |
    | E6/55                            |                       |            |              | MPQ5_TX2N                      |                                        |
    | E8/55                            |                       |            |              | MPQ5_TX0P                      |                                        |
    | E9/55                            |                       |            |              | MPQ5_TX0N                      |                                        |
    | E11/54                           |                       |            |              | MPQ4_TX2P                      |                                        |
    | E12/54                           |                       |            |              | MPQ4_TX2N                      |                                        |
    | E14/54                           |                       |            |              | MPQ4_TX0P                      |                                        |
    | E15/54                           |                       |            |              | MPQ4_TX0N                      |                                        |
    | E17/53                           |                       |            |              | MPQ3_TX2P                      |                                        |
    | E18/53                           |                       |            |              | MPQ3_TX2N                      |                                        |
    | E20/53                           |                       |            |              | MPQ3_TX0P                      |                                        |
    | E21/53                           |                       |            |              | MPQ3_TX0N                      |                                        |
    | E23/52                           |                       |            |              | MPQ2_TX2P                      |                                        |
    | E24/52                           |                       |            |              | MPQ2_TX2N                      |                                        |
    | E26/52                           |                       |            |              | MPQ2_TX0P                      |                                        |
    | E27/52                           |                       |            |              | MPQ2_TX0N                      |                                        |
    | E29/51                           |                       |            |              | MPQ1_TX2P                      |                                        |
    | E30/51                           |                       |            |              | MPQ1_TX2N                      |                                        |
    | E32/51                           |                       |            |              | MPQ1_TX0P                      |                                        |
    | E33/51                           |                       |            |              | MPQ1_TX0N                      |                                        |
    | F1/56                            |                       |            |              | MPQ6_RX2P                      |                                        |
    | F3/56                            |                       |            |              | MPQ6_RX3P                      |                                        |
    | G5/55                            |                       |            |              | MPQ5_TX3P                      |                                        |
    | G6/55                            |                       |            |              | MPQ5_TX3N                      |                                        |
    | G8/55                            |                       |            |              | MPQ5_TX1P                      |                                        |
    | G9/55                            |                       |            |              | MPQ5_TX1N                      |                                        |
    | G11/54                           |                       |            |              | MPQ4_TX3P                      |                                        |
    | G12/54                           |                       |            |              | MPQ4_TX3N                      |                                        |
    | G14/54                           |                       |            |              | MPQ4_TX1P                      |                                        |
    | G15/54                           |                       |            |              | MPQ4_TX1N                      |                                        |
    | G17/53                           |                       |            |              | MPQ3_TX3P                      |                                        |
    | G18/53                           |                       |            |              | MPQ3_TX3N                      |                                        |
    | G20/53                           |                       |            |              | MPQ3_TX1P                      |                                        |
    | G21/53                           |                       |            |              | MPQ3_TX1N                      |                                        |
    | G23/52                           |                       |            |              | MPQ2_TX3P                      |                                        |
    | G24/52                           |                       |            |              | MPQ2_TX3N                      |                                        |
    | G26/52                           |                       |            |              | MPQ2_TX1P                      |                                        |
    | G27/52                           |                       |            |              | MPQ2_TX1N                      |                                        |
    | G29/51                           |                       |            |              | MPQ1_TX3P                      |                                        |
    | G30/51                           |                       |            |              | MPQ1_TX3N                      |                                        |
    | G32/51                           |                       |            |              | MPQ1_TX1P                      |                                        |
    | G33/51                           |                       |            |              | MPQ1_TX1N                      |                                        |
    | H1/56                            |                       |            |              | MPQ6_TX0N                      |                                        |
    | H3/56                            |                       |            |              | MPQ6_TX1N                      |                                        |
    | HPIO_BANK_PVTCAL_CORE_R115C101/0 |                       |            |              | HPIO_BANK_PVTCAL_CORE_R115C101 |                                        |
    | HPIO_BANK_PVTCAL_CORE_R115C145/0 |                       |            |              | HPIO_BANK_PVTCAL_CORE_R115C145 |                                        |
    | HPIO_BANK_PVTCAL_CORE_R115C186/0 |                       |            |              | HPIO_BANK_PVTCAL_CORE_R115C186 |                                        |
    | HPIO_BANK_PVTCAL_CORE_R115C221/0 |                       |            |              | HPIO_BANK_PVTCAL_CORE_R115C221 |                                        |
    | HPIO_BANK_PVTCAL_CORE_R115C25/0  |                       |            |              | HPIO_BANK_PVTCAL_CORE_R115C25  |                                        |
    | HPIO_BANK_PVTCAL_CORE_R115C265/0 |                       |            |              | HPIO_BANK_PVTCAL_CORE_R115C265 |                                        |
    | HPIO_BANK_PVTCAL_CORE_R115C306/0 |                       |            |              | HPIO_BANK_PVTCAL_CORE_R115C306 |                                        |
    | HPIO_BANK_PVTCAL_CORE_R115C341/0 |                       |            |              | HPIO_BANK_PVTCAL_CORE_R115C341 |                                        |
    | HPIO_BANK_PVTCAL_CORE_R115C66/0  |                       |            |              | HPIO_BANK_PVTCAL_CORE_R115C66  |                                        |
    | HPIO_DFTCIB_R115C209/0           |                       |            |              | HPIO_DFTCIB_R115C209           |                                        |
    | HPIO_DFTCIB_R115C329/0           |                       |            |              | HPIO_DFTCIB_R115C329           |                                        |
    | HPIO_DFTCIB_R115C89/0            |                       |            |              | HPIO_DFTCIB_R115C89            |                                        |
    | HPIO_DFTMUX_SECTOR_3/0           |                       |            |              | HPIO_DFTMUX_SECTOR_3           |                                        |
    | HPIO_DFTMUX_SECTOR_6/0           |                       |            |              | HPIO_DFTMUX_SECTOR_6           |                                        |
    | HPIO_DFTMUX_SECTOR_9/0           |                       |            |              | HPIO_DFTMUX_SECTOR_9           |                                        |
    | J1/56                            |                       |            |              | MPQ6_TX0P                      |                                        |
    | J3/56                            |                       |            |              | MPQ6_TX1P                      |                                        |
    | J8/55                            |                       |            |              | MPQ5_REFCLKP                   |                                        |
    | J9/55                            |                       |            |              | MPQ5_REFCLKN                   |                                        |
    | J14/54                           |                       |            |              | MPQ4_REFCLKN                   |                                        |
    | J15/54                           |                       |            |              | MPQ4_REFCLKP                   |                                        |
    | J20/53                           |                       |            |              | MPQ3_REFCLKN                   |                                        |
    | J21/53                           |                       |            |              | MPQ3_REFCLKP                   |                                        |
    | J26/52                           |                       |            |              | MPQ2_REFCLKP                   |                                        |
    | J27/52                           |                       |            |              | MPQ2_REFCLKN                   |                                        |
    | J32/51                           |                       |            |              | MPQ1_REFCLKP                   |                                        |
    | J33/51                           |                       |            |              | MPQ1_REFCLKN                   |                                        |
    | K5/56                            |                       |            |              | MPQ6_REFCLKN                   |                                        |
    | L1/56                            |                       |            |              | MPQ6_TX2N                      |                                        |
    | L3/56                            |                       |            |              | MPQ6_TX3N                      |                                        |
    | L5/56                            |                       |            |              | MPQ6_REFCLKP                   |                                        |
    | L7/1                             |     unused, PULL:DOWN |            |              | WRIO1_4A                       | MDQ4/UMDQ1_4                           |
    | L8/1                             |     unused, PULL:DOWN |            |              | WRIO1_4B                       | MDQ5/UMDQ1_5                           |
    | L9/1                             |     unused, PULL:DOWN |            |              | WRIO1_2B                       | MDQ3/UMDQ1_3                           |
    | L10/1                            |     unused, PULL:DOWN |            |              | WRIO1_2A                       | MDQ2/UMDQ1_2                           |
    | L11/1                            | Reserved: sysCONFIG   |            |              | WRIO1_0B                       | MDQ1/UMDQ1_1                           |
    | L12/1                            | Reserved: sysCONFIG   |            |              | WRIO1_0A                       | MDQ0/UMDQ1_0                           |
    | L28/50                           |                       |            |              | MPQ0_TX3P                      |                                        |
    | L30/50                           |                       |            |              | MPQ0_TX2P                      |                                        |
    | L32/50                           |                       |            |              | MPQ0_RX3P                      |                                        |
    | L34/50                           |                       |            |              | MPQ0_RX2P                      |                                        |
    | M1/56                            |                       |            |              | MPQ6_TX2P                      |                                        |
    | M3/56                            |                       |            |              | MPQ6_TX3P                      |                                        |
    | M8/1                             |     unused, PULL:DOWN |            |              | WRIO1_6A                       | MDQ6/UMDQ1_6                           |
    | M9/1                             |     unused, PULL:DOWN |            |              | WRIO1_6B                       | MDQ7/UMDQ1_7                           |
    | M19/12                           |     unused, PULL:DOWN |            |              | WRIO12_3A                      | UMCSN12                                |
    | M20/12                           |     unused, PULL:DOWN |            |              | WRIO12_3B                      | PCLKT12_0/PCLKRT12_0/UMDS12            |
    | M28/50                           |                       |            |              | MPQ0_TX3N                      |                                        |
    | M30/50                           |                       |            |              | MPQ0_TX2N                      |                                        |
    | M32/50                           |                       |            |              | MPQ0_RX3N                      |                                        |
    | M34/50                           |                       |            |              | MPQ0_RX2N                      |                                        |
    | N5/2                             |     unused, PULL:DOWN |            |              | WRIO2_0B                       | SDQ1/USDQ2_1                           |
    | N6/2                             |     unused, PULL:DOWN |            |              | WRIO2_0A                       | SDQ0/USDQ2_0                           |
    | N7/1                             |     unused, PULL:DOWN |            |              | WRIO1_3B                       | PCLKRT1_0/MDS/UMDS1                    |
    | N10/1                            |     unused, PULL:DOWN |            |              | WRIO1_7B                       | W_PLLMFGOUT2                           |
    | N14/12                           |     unused, PULL:DOWN |            |              | WRIO12_0B                      | UMDQ12_1                               |
    | N15/12                           |     unused, PULL:DOWN |            |              | WRIO12_0A                      | UMDQ12_0                               |
    | N16/12                           |     unused, PULL:DOWN |            |              | WRIO12_2B                      | UMDQ12_3                               |
    | N17/12                           |     unused, PULL:DOWN |            |              | WRIO12_1B                      | PCLKT12_1/PCLKRT12_1                   |
    | N19/12                           |     unused, PULL:DOWN |            |              | WRIO12_1A                      |                                        |
    | N20/12                           |     unused, PULL:DOWN |            |              | WRIO12_5B                      | UMCK12N                                |
    | N26/50                           |                       |            |              | MPQ0_REFCLKN                   |                                        |
    | P3/2                             |     unused, PULL:DOWN |            |              | WRIO2_4A                       | SDQ4/USDQ2_4                           |
    | P4/2                             |     unused, PULL:DOWN |            |              | WRIO2_4B                       | SDQ5/USDQ2_5                           |
    | P5/2                             |     unused, PULL:DOWN |            |              | WRIO2_2B                       | SDQ3/USDQ2_3                           |
    | P6/2                             |     unused, PULL:DOWN |            |              | WRIO2_2A                       | SDQ2/USDQ2_2                           |
    | P7/1                             | Reserved: sysCONFIG   |            |              | WRIO1_3A                       | MCSN/UMCSN1                            |
    | P8/1                             |     unused, PULL:DOWN |            |              | WRIO1_5B                       | MCLKN/UMCK1N                           |
    | P9/1                             | Reserved: sysCONFIG   |            |              | WRIO1_5A                       | MCLKP/UMCK1P                           |
    | P10/1                            |     unused, PULL:DOWN |            |              | WRIO1_7A                       | W_PLLMFGOUT1/MRSTN/UMRSTN1             |
    | P13/12                           |     unused, PULL:DOWN |            |              | WRIO12_4A                      | UMDQ12_4                               |
    | P14/12                           |     unused, PULL:DOWN |            |              | WRIO12_4B                      | UMDQ12_5                               |
    | P15/12                           |     unused, PULL:DOWN |            |              | WRIO12_2A                      | UMDQ12_2                               |
    | P18/12                           |     unused, PULL:DOWN |            |              | WRIO12_7B                      | PLLTFB12_IN                            |
    | P19/12                           |     unused, PULL:DOWN |            |              | WRIO12_7A                      | PLLT12_IN                              |
    | P20/12                           |     unused, PULL:DOWN |            |              | WRIO12_5A                      | UMCK12P                                |
    | P26/50                           |                       |            |              | MPQ0_REFCLKP                   |                                        |
    | P28/50                           |                       |            |              | MPQ0_TX1P                      |                                        |
    | P30/50                           |                       |            |              | MPQ0_TX0P                      |                                        |
    | P32/50                           |                       |            |              | MPQ0_RX1P                      |                                        |
    | P34/50                           |                       |            |              | MPQ0_RX0P                      |                                        |
    | R1/2                             | Reserved: sysCONFIG   |            |              | WRIO2_7B                       | TMS                                    |
    | R3/2                             |     unused, PULL:DOWN |            |              | WRIO2_6A                       | SDQ6/USDQ2_6                           |
    | R5/2                             |     unused, PULL:DOWN |            |              | WRIO2_3B                       | SDS/USDS2                              |
    | R6/2                             |     unused, PULL:DOWN |            |              | WRIO2_3A                       | SCSN/USCSN2                            |
    | R8/1                             |     unused, PULL:DOWN |            |              | WRIO1_1B                       | MSDO/MCSNO                             |
    | R9/14                            |     unused, PULL:DOWN |            |              | WRIO14_8B                      |                                        |
    | R10/14                           |     unused, PULL:DOWN |            |              | WRIO14_9B                      |                                        |
    | R11/14                           |     unused, PULL:DOWN |            |              | WRIO14_9A                      |                                        |
    | R12/14                           |     unused, PULL:DOWN |            |              | WRIO14_7A                      |                                        |
    | R13/13                           | sw15                  | LOCATED    | LVCMOS33_IN  | WRIO13_7B                      | U_PLLMFGOUT2                           |
    | R14/13                           | seg3                  | LOCATED    | LVCMOS33_OUT | WRIO13_1A                      |                                        |
    | R15/13                           | seg_dp                | LOCATED    | LVCMOS33_OUT | WRIO13_1B                      |                                        |
    | R16/12                           |     unused, PULL:DOWN |            |              | WRIO12_6A                      | UMDQ12_6                               |
    | R17/12                           |     unused, PULL:DOWN |            |              | WRIO12_6B                      | UMDQ12_7                               |
    | R18/13                           | seg2                  | LOCATED    | LVCMOS33_OUT | WRIO13_0B                      | UMDQ13_1                               |
    | R19/13                           | seg1                  | LOCATED    | LVCMOS33_OUT | WRIO13_0A                      | UMDQ13_0                               |
    | R28/50                           |                       |            |              | MPQ0_TX1N                      |                                        |
    | R30/50                           |                       |            |              | MPQ0_TX0N                      |                                        |
    | R32/50                           |                       |            |              | MPQ0_RX1N                      |                                        |
    | R34/50                           |                       |            |              | MPQ0_RX0N                      |                                        |
    | T1/2                             | Reserved: sysCONFIG   |            |              | WRIO2_7A                       | TCK                                    |
    | T3/2                             |     unused, PULL:DOWN |            |              | WRIO2_6B                       | SDQ7/USDQ2_7                           |
    | T6/0                             |     unused, PULL:DOWN |            |              | WRIO0_7B                       | PLLTFB0_IN                             |
    | T7/0                             | clk_in                | LOCATED    | LVCMOS33_IN  | WRIO0_3B                       | PCLKT0_0/PCLKRT0_0/UMDS0               |
    | T8/0                             |     unused, PULL:DOWN |            |              | WRIO0_1B                       | PCLKT0_1/PCLKRT0_1                     |
    | T9/14                            |     unused, PULL:DOWN |            |              | WRIO14_8A                      |                                        |
    | T10/14                           |     unused, PULL:DOWN |            |              | WRIO14_0B                      | USDQ14_1                               |
    | T11/14                           |     unused, PULL:DOWN |            |              | WRIO14_7B                      |                                        |
    | T12/14                           |     unused, PULL:DOWN |            |              | WRIO14_5B                      |                                        |
    | T13/13                           | sw14                  | LOCATED    | LVCMOS33_IN  | WRIO13_7A                      | U_PLLMFGOUT1                           |
    | T15/13                           | seg_c                 | LOCATED    | LVCMOS33_OUT | WRIO13_3A                      | UMCSN13                                |
    | T18/13                           | seg_a                 | LOCATED    | LVCMOS33_OUT | WRIO13_2A                      | UMDQ13_2                               |
    | T19/13                           | seg_b                 | LOCATED    | LVCMOS33_OUT | WRIO13_2B                      | UMDQ13_3                               |
    | T24/11                           |     unused, PULL:DOWN |            |              | HPIO11_20B                     | DQ11_2                                 |
    | T25/11                           |     unused, PULL:DOWN |            |              | HPIO11_14B                     | DQ11_2                                 |
    | T26/11                           |     unused, PULL:DOWN |            |              | HPIO11_12A                     | VREF11                                 |
    | U1/2                             | Reserved: sysCONFIG   |            |              | WRIO2_9A                       | TDI                                    |
    | U2/2                             | Reserved: sysCONFIG   |            |              | WRIO2_9B                       | TDO                                    |
    | U3/2                             |     unused, PULL:DOWN |            |              | WRIO2_5A                       | PCLKRT2_0/SCLKP/USCK2P                 |
    | U5/2                             |     unused, PULL:DOWN |            |              | WRIO2_1B                       | SSDO                                   |
    | U6/0                             |     unused, PULL:DOWN |            |              | WRIO0_7A                       | PLLT0_IN                               |
    | U7/0                             |     unused, PULL:DOWN |            |              | WRIO0_3A                       | UMCSN0                                 |
    | U8/0                             |     unused, PULL:DOWN |            |              | WRIO0_1A                       |                                        |
    | U12/14                           |     unused, PULL:DOWN |            |              | WRIO14_5A                      | PCLKRT14_0/USCK14P                     |
    | U15/13                           |     unused, PULL:DOWN |            |              | WRIO13_3B                      | PCLKRT13_0/UMDS13                      |
    | U16/13                           | seg_d                 | LOCATED    | LVCMOS33_OUT | WRIO13_4A                      | UMDQ13_4                               |
    | U17/13                           | seg_e                 | LOCATED    | LVCMOS33_OUT | WRIO13_4B                      | UMDQ13_5                               |
    | U22/11                           |     unused, PULL:DOWN |            |              | HPIO11_22B                     | DQ11_2                                 |
    | U23/11                           |     unused, PULL:DOWN |            |              | HPIO11_22A                     | DQ11_2                                 |
    | U24/11                           |     unused, PULL:DOWN |            |              | HPIO11_20A                     | DQ11_2                                 |
    | U25/11                           |     unused, PULL:DOWN |            |              | HPIO11_14A                     | DQ11_2                                 |
    | U26/11                           | Prohibited/Reserved   |            |              | HPIO11_12B                     | EXT_RES11                              |
    | U27/11                           |     unused, PULL:DOWN |            |              | HPIO11_4A                      | DQS11_0                                |
    | U28/11                           |     unused, PULL:DOWN |            |              | HPIO11_2B                      | DQ11_0                                 |
    | U29/11                           |     unused, PULL:DOWN |            |              | HPIO11_3A                      | DQ11_1                                 |
    | U30/11                           |     unused, PULL:DOWN |            |              | HPIO11_9A                      | DQ11_1                                 |
    | U31/11                           |     unused, PULL:DOWN |            |              | HPIO11_9B                      | DQ11_1                                 |
    | U32/11                           |     unused, PULL:DOWN |            |              | HPIO11_13B                     | PLLC11_IN                              |
    | U33/11                           |     unused, PULL:DOWN |            |              | HPIO11_13A                     | PLLT11_IN                              |
    | U34/11                           |     unused, PULL:DOWN |            |              | HPIO11_17A                     | SD1_IN/DQ11_3                          |
    | V1/0                             |     unused, PULL:DOWN |            |              | WRIO0_4B                       | UMDQ0_5                                |
    | V2/0                             |     unused, PULL:DOWN |            |              | WRIO0_6A                       | UMDQ0_6                                |
    | V4/0                             |     unused, PULL:DOWN |            |              | WRIO0_2A                       | UMDQ0_2                                |
    | V5/0                             |     unused, PULL:DOWN |            |              | WRIO0_0B                       | UMDQ0_1                                |
    | V8/14                            |     unused, PULL:DOWN |            |              | WRIO14_6A                      | USDQ14_6                               |
    | V9/14                            |     unused, PULL:DOWN |            |              | WRIO14_4B                      | USDQ14_5                               |
    | V10/14                           |     unused, PULL:DOWN |            |              | WRIO14_0A                      | USDQ14_0                               |
    | V11/14                           |     unused, PULL:DOWN |            |              | WRIO14_2B                      | USDQ14_3                               |
    | V12/14                           |     unused, PULL:DOWN |            |              | WRIO14_1A                      |                                        |
    | V13/14                           |     unused, PULL:DOWN |            |              | WRIO14_1B                      |                                        |
    | V14/13                           | seg_g                 | LOCATED    | LVCMOS33_OUT | WRIO13_5B                      | UMCK13N                                |
    | V15/13                           | sw13                  | LOCATED    | LVCMOS33_IN  | WRIO13_6B                      | UMDQ13_7                               |
    | V16/13                           | sw12                  | LOCATED    | LVCMOS33_IN  | WRIO13_6A                      | UMDQ13_6                               |
    | V22/11                           |     unused, PULL:DOWN |            |              | HPIO11_24A                     | PCLKRT11_2/PCLKET11_2/DM11_2           |
    | V25/11                           |     unused, PULL:DOWN |            |              | HPIO11_10A                     | PCLKT11_0/PCLKRT11_0/PCLKET11_0/DM11_0 |
    | V26/11                           |     unused, PULL:DOWN |            |              | HPIO11_8B                      | DQ11_0                                 |
    | V27/11                           |     unused, PULL:DOWN |            |              | HPIO11_4B                      | DQSN11_0                               |
    | V28/11                           |     unused, PULL:DOWN |            |              | HPIO11_2A                      | DQ11_0                                 |
    | V29/11                           |     unused, PULL:DOWN |            |              | HPIO11_3B                      | DQ11_1                                 |
    | V30/11                           |     unused, PULL:DOWN |            |              | HPIO11_7A                      | DQ11_1                                 |
    | V31/11                           |     unused, PULL:DOWN |            |              | HPIO11_11B                     | PCLKC11_1/PCLKRC11_1/PCLKEC11_1        |
    | V32/11                           |     unused, PULL:DOWN |            |              | HPIO11_11A                     | PCLKT11_1/PCLKRT11_1/PCLKET11_1/DM11_1 |
    | V33/11                           |     unused, PULL:DOWN |            |              | HPIO11_15A                     | DQ11_3                                 |
    | V34/11                           |     unused, PULL:DOWN |            |              | HPIO11_17B                     | SD1_OUT/DQ11_3                         |
    | W1/0                             |     unused, PULL:DOWN |            |              | WRIO0_4A                       | UMDQ0_4                                |
    | W2/0                             |     unused, PULL:DOWN |            |              | WRIO0_6B                       | UMDQ0_7                                |
    | W4/0                             |     unused, PULL:DOWN |            |              | WRIO0_2B                       | UMDQ0_3                                |
    | W5/0                             |     unused, PULL:DOWN |            |              | WRIO0_0A                       | UMDQ0_0                                |
    | W6/0                             |     unused, PULL:DOWN |            |              | WRIO0_5B                       | UMCK0N                                 |
    | W7/0                             |     unused, PULL:DOWN |            |              | WRIO0_5A                       | UMCK0P                                 |
    | W8/14                            |     unused, PULL:DOWN |            |              | WRIO14_6B                      | USDQ14_7                               |
    | W9/14                            |     unused, PULL:DOWN |            |              | WRIO14_4A                      | USDQ14_4                               |
    | W10/14                           |     unused, PULL:DOWN |            |              | WRIO14_2A                      | USDQ14_2                               |
    | W11/14                           |     unused, PULL:DOWN |            |              | WRIO14_3B                      | USDS14                                 |
    | W12/14                           |     unused, PULL:DOWN |            |              | WRIO14_3A                      | USCSN14                                |
    | W14/13                           | seg_f                 | LOCATED    | LVCMOS33_OUT | WRIO13_5A                      | UMCK13P                                |
    | W22/11                           |     unused, PULL:DOWN |            |              | HPIO11_24B                     | PCLKRC11_2/PCLKEC11_2                  |
    | W23/11                           |     unused, PULL:DOWN |            |              | HPIO11_18A                     | DQS11_2                                |
    | W24/11                           |     unused, PULL:DOWN |            |              | HPIO11_18B                     | DQSN11_2                               |
    | W25/11                           |     unused, PULL:DOWN |            |              | HPIO11_10B                     | PCLKC11_0/PCLKRC11_0/PCLKEC11_0        |
    | W26/11                           |     unused, PULL:DOWN |            |              | HPIO11_8A                      | HS11_PLL_MFGOUT2/DQ11_0                |
    | W29/11                           |     unused, PULL:DOWN |            |              | HPIO11_5B                      | DQSN11_1                               |
    | W30/11                           |     unused, PULL:DOWN |            |              | HPIO11_7B                      | DQ11_1                                 |
    | W33/11                           |     unused, PULL:DOWN |            |              | HPIO11_15B                     | DQ11_3                                 |
    | W34/11                           |     unused, PULL:DOWN |            |              | HPIO11_19B                     | DQSN11_3                               |
    | Y1/3                             |     unused, PULL:DOWN |            |              | HPIO3_13A                      | PLLT3_IN                               |
    | Y2/3                             |     unused, PULL:DOWN |            |              | HPIO3_15B                      | DQ3_3                                  |
    | Y3/3                             |     unused, PULL:DOWN |            |              | HPIO3_17B                      | SD13_OUT/DQ3_3                         |
    | Y4/3                             |     unused, PULL:DOWN |            |              | HPIO3_21B                      | SD17_OUT/DQ3_3                         |
    | Y5/3                             |     unused, PULL:DOWN |            |              | HPIO3_23A                      | DQ3_3                                  |
    | Y6/3                             |     unused, PULL:DOWN |            |              | HPIO3_25B                      | PCLKRC3_3/PCLKEC3_3                    |
    | Y7/3                             |     unused, PULL:DOWN |            |              | HPIO3_25A                      | PCLKRT3_3/PCLKET3_3/DM3_3              |
    | Y8/3                             |     unused, PULL:DOWN |            |              | HPIO3_16A                      | SD12_IN/DQ3_2                          |
    | Y9/3                             |     unused, PULL:DOWN |            |              | HPIO3_16B                      | SD12_OUT/DQ3_2                         |
    | Y10/3                            |     unused, PULL:DOWN |            |              | HPIO3_14B                      | DQ3_2                                  |
    | Y11/3                            |     unused, PULL:DOWN |            |              | HPIO3_14A                      | DQ3_2                                  |
    | Y17/7                            |     unused, PULL:DOWN |            |              | HPIO7_2A                       | DQ7_0                                  |
    | Y18/7                            |     unused, PULL:DOWN |            |              | HPIO7_2B                       | DQ7_0                                  |
    | Y20/8                            |     unused, PULL:DOWN |            |              | HPIO8_2A                       | DQ8_0                                  |
    | Y21/10                           |     unused, PULL:DOWN |            |              | HPIO10_22A                     | DQ10_2                                 |
    | Y24/11                           |     unused, PULL:DOWN |            |              | HPIO11_16B                     | SD0_OUT/DQ11_2                         |
    | Y26/11                           |     unused, PULL:DOWN |            |              | HPIO11_6B                      | DQ11_0                                 |
    | Y27/11                           |     unused, PULL:DOWN |            |              | HPIO11_0B                      | DQ11_0                                 |
    | Y28/11                           |     unused, PULL:DOWN |            |              | HPIO11_1A                      | DQ11_1                                 |
    | Y29/11                           |     unused, PULL:DOWN |            |              | HPIO11_5A                      | DQS11_1                                |
    | Y30/11                           |     unused, PULL:DOWN |            |              | HPIO11_23B                     | DQ11_3                                 |
    | Y31/11                           |     unused, PULL:DOWN |            |              | HPIO11_23A                     | DQ11_3                                 |
    | Y32/11                           |     unused, PULL:DOWN |            |              | HPIO11_21A                     | DQ11_3                                 |
    | Y33/11                           |     unused, PULL:DOWN |            |              | HPIO11_21B                     | DQ11_3                                 |
    | Y34/11                           |     unused, PULL:DOWN |            |              | HPIO11_19A                     | DQS11_3                                |
    +----------------------------------+-----------------------+------------+--------------+--------------------------------+----------------------------------------+

    sysCONFIG Pins:
    +----------+--------------------+----------+-------------+
    | Pad Name | sysCONFIG Pin Name | Pin/Bank | Buffer Type |
    +----------+--------------------+----------+-------------+
    | WRIO1_0B | MDQ1/UMDQ1_1       | L11/1    |             |
    | WRIO1_0A | MDQ0/UMDQ1_0       | L12/1    |             |
    | WRIO1_3A | MCSN/UMCSN1        | P7/1     |             |
    | WRIO1_5A | MCLKP/UMCK1P       | P9/1     |             |
    | WRIO2_1A | INITN              | T5/2     |             |
    | WRIO2_5B | DONE               | U4/2     |             |
    | WRIO2_7B | TMS                | R1/2     |             |
    | WRIO2_7A | TCK                | T1/2     |             |
    | WRIO2_8B | PROGRAMN           | P2/2     |             |
    | WRIO2_9B | TDO                | U2/2     |             |
    | WRIO2_9A | TDI                | U1/2     |             |
    +----------+--------------------+----------+-------------+

    Locate Constraints for each Pin:

    ldc_set_location -site {T7} [ get_ports {clk_in} ]
    ldc_set_location -site {R19} [ get_ports {seg1} ]
    ldc_set_location -site {R18} [ get_ports {seg2} ]
    ldc_set_location -site {R14} [ get_ports {seg3} ]
    ldc_set_location -site {T18} [ get_ports {seg_a} ]
    ldc_set_location -site {T19} [ get_ports {seg_b} ]
    ldc_set_location -site {T15} [ get_ports {seg_c} ]
    ldc_set_location -site {U16} [ get_ports {seg_d} ]
    ldc_set_location -site {R15} [ get_ports {seg_dp} ]
    ldc_set_location -site {U17} [ get_ports {seg_e} ]
    ldc_set_location -site {W14} [ get_ports {seg_f} ]
    ldc_set_location -site {V14} [ get_ports {seg_g} ]
    ldc_set_location -site {V16} [ get_ports {sw12} ]
    ldc_set_location -site {V15} [ get_ports {sw13} ]
    ldc_set_location -site {T13} [ get_ports {sw14} ]
    ldc_set_location -site {R13} [ get_ports {sw15} ]

    #PLL
    ldc_set_location -site {PLL11} [ get_cells {pll_inst.lscc_pll_inst.gen_ext_outclkdiv.gen_no_clk7.u_pll.PLLC_MODE_inst} ]

    Copyright (c) 2002-2022 Lattice Semiconductor Corporation,  All rights reserved.

    Thu Mar 14 15:43:21 2024